**Scope 4.6 Hauling Services Specifications**

* Vendor will drop off container on project site (roll on, roll off system);
* Container must be capable of holding woody biomass (chipped or unchipped; but not in the same container);
* Available container volumes should be ten (10), twenty (20), and thirty (30) cubic yards, or volume specified by State’s designee; and
* The containers will be hauled by the vendor from project sites to landfills, power plants, or biomass recycling centers on specially constructed heavy trucks.
* Vendor may be requested to remove previously cut fuel wood from a project site.