**Scope 4.2 Large Tree Removal Services Specification**

* Class A: Any tree that can be laid down with a clear path on said property. (e.g., A 200’ tree or a 30’ tree regardless of the height and diameter, if the tree has a clear path to fall and can be easily topped and limbed. This job would require one (1) or more people);
* Class B: Any tree needing to be climbed, trimmed, topped and pieced out. (This job requires one (1) climber/faller and one (1) or more ground person); and
* Class C: Mechanical involvement required. (e.g., Crane job – 100’ crane. This job would require two (2) or more people).